Optimization in VLSI digital circuits is required in order to design an efficient circuit in terms of area and power.

In combinational circuit design optimization is done at two levels.

- Constant propagation

- Boolean logic optimization

Combinational circuits with constant propagation:

Let consider an the following combinational circuit: